	■
Original Request
	Sample No.
Type of Cigarctte
Batch Size
	6030
85 mm Filter
50 lbs.

	
	Made By
	Dr. A. W. Spc
	•ars	on September 21
	,1976

	Sample Specifications Written By	W. E
	:.Rou th
	
	

	
	
	
	
	•
	Additional

	BLEND
	CASING
	RECASING
	FINAL FLAVOR
	
	

	OGS
	
	OGS
	OGS
	OGS
	3.4%
	PMO in

	Ciqarettos
	
	•
	
	FiltCfS
	
	

	Maker
	AMF
	
	
	Kind 20 mm True plastic
	rod

	Length
	85 mm
	
	
	
	

	Circumference
	25.0
	
	Process
	
	

	Weight To be
	det. (803
	mq tobacco)
	Rod Length
	
	

	Pressure Drop
	To be determined
	Pressure Drop
	
	

	Filter Length
	20 nun
	
	Circumference
	
	

	Paper
	
	554
	
	i Weight
	
	

	Tipping Paper
	30 nun
	
	Plasticizer
	
	

	
	
	
	
	Plug \lrav)
	
	

	
	
	
	■
	•Responsibility
	
	

	Labels
	
	Wh i tie
	
	Tobacco Blend
	Ammons
	

	Closures
	
	Blue
	
	Filter Production
	Wicker
	

	.• Tear Tape
	
	Whi te
	
	Making & Packing
	Brown ,/Rou til

	Cartons
	
	u
	
	Shipping
	Routh
	

	Markings
	Sample No. on
	Sample Requisition
	
	

	
	overwrcip
	
	[Form 02:02:06]
	
	

	Requirements
	
	
	
	Special Requirements
	
	•


Date:	AopLcnUx.'r 2],['丿
Spray
Eton



Laboratory 3 cartons Other	36~7OOO ciqts.
Laboratory Analysis
一-—	-smoke Analysis
PMO Analysis Spray 50 lbs. tobacco with solution of 880 g (= 1.94 lbs.) PMO in 1175 ml of denatured alcohol. This should give 3.4$ PMO add-on (3.3% PMO contained) assuming 88% spraying efficiency. PMO deliver.y from 85 nun cigarette smoked to 30 mm butt should be 6.5 mg/cig.


Dr. F. J.,SrhnLtz_ Dr. H. J. Mi nnemever
00003726

Reports
Written by P. D. Schiukcdantz
Original to Dr.八.W. Spcai: ~~~ Copies to


Managed, kxisiixcctx
Research
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