Date: September 21, 1976
	Sample No.
	6030

	Type of Cigarette
	85 mm Filter

	Batch Size
	50 1bs.


Original Request Made By Dr. A. W. Spears on September 21, 1976
Sample Specifications Written By W. E. Routh .
	BLEND
	CASING
	RECASING
	FINAL FLAVOR
	Additional Spray XEXXXXXXX

	OGS
	OGS
	OGS
	OGS
	3.4% PMO in EtoH



	Cigarettes
	Maker AMF
	

	Length 85
	mm

	Circumference
	25.0

	Weight To be
	det. (803 mq tobacco)

	Pressure Drop
	To be determined

	Filter Length
	20 mm

	Paper
	554

	Tipping Paper
	30 mm


epping
	Labels
	White

	Closures
	Blue

	Tear Tape
	White

	Cartons
	"

	Markings
	Sample No. on

	
	overwrap


Requirements
Laboratory 3 cartons
Other 20,000 cigts.
Laboratory Analysis
Smoke Analysis
PMO Analysis
Reports
	Written by
	P.
	D.
	
	Schickedantz

	Original to
	Dr.
	A. W.
	Spears

	Copies to
	Dr.
	F. J.
	Schultz

	
	Dr.
	H. J.
	Minnemever

	

	
	
	
	

	
	
	



	Filters
Kind	20 mm True plastic rod
Process
Rod Length
Pressure Drop
Circumference
weight
Plasticizer
Plug Wrap
Responsibility
Tobacco Blend Ammons
Filter Production Wicker
Making & Packing	Brown/Routh
Shipping Routh
.
Sample Requisition [Form 02:02:06]
Special Requirements
Spray 50 lbs. tobacco with solution of 880 g (= 1.94 lbs.) PMO in 1175 ml of denatured alcohol. This should give 3.4% PMO add-on (3.3% PMO contained) assuming 88% spraying efficiency. PMO delivery from 85 mm cigarette smoked to 30 mm butt should be 6.5 mg/cig.
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